
 This is SB16MIX FAQ (Frequently Asked Questions):
 -------------------------------------------------

Q: I have 16 bit sound card, but SB16MIX complains SB16 is not detected. Why?
A: 16 bit does not mean SB16. Read the manual of your card to check if your
   sound card is really SB16 compatible (if was cheap, probably isn't).

Q: Is possible to use this program as mixer control in Windows?
A: Not fully. You can run this program in Windows, but when is running, sound
   card is blocked and no other program can access it. 

Q: I started SB16MIX under Windows and it can't detect my SB 32 AWE. Why?
A: Because other programs is using your sound card. Close them and try again.

Q: I clicked on Mixer Reset and nothing happened. Why?
A: a) Your sound card is slow, read the doc for more info.
   b) Because the mixer state does not changed since hardware reset of sound
      card. Try to change something and click again.

Q: When I tried to change recording source selection, nothing changed. Why?
A: Your recording program overrided it. You have to use a program, which does
   not set recording source by default, for example WREC and VREC by Creative
   Labs, supplied with SB16 (or from SB_DISK.ZIP package, available on FTPs).

Q: When I start SB16MIX, it displays message and wait about one second. Why?
A: You have old mouse driver, that does not support fast software reser of
   mouse and program has to use hardware mouse reset. It means mouse poweroff
   and this is quite slow process (the driver has to wait for discharge of all
   capacitors in mouse). Solution: Upgrade your mouse driver.
